**Kalyan Dombivli Municipal Corporation**  
**Construction, Kalyan Department**  
Ref. No.: JAKRA/KANDOMPA/KAA /BANDH/KAVI/25  
Date: 02/05/2025

To,

M/s, Bharati Airtel Ltd.

7th Floor Interface 07, New link road,

Malad West, Mumbai – 400 064

**Subject:** Permission for laying OFC cable in Kalyan Division for M/s Bharti Airtel Ltd.  
**Reference:** 1) Application from M/s Bharti Airtel Ltd. dated 25/04/2025.

2) Hons. City Engineer D, Approval on 25/04/2025.

As per the subject mentioned above, M/s Bharti Airtel Ltd. is expected to be granted permission to lay OFC cable in the Kalyan Division. According to the reference letter, M/s Bharti Airtel Ltd. has requested permission for laying OFC cable for a total length of 130.00 meters of road work, with the details as follows:

| **Sr. No.** | **Road Name** | **Division** | **Length Paver Block (meters)** | **Total Length (meters)** |
| --- | --- | --- | --- | --- |
| 1 | Bhiwandi Murbad - road shriganesh Vandan Building to hotel Sai Daba | Kalyan | 130 | 130 |

**Total Paver Block – 130 Meter**

**Table A:**

| **Sr. No.** | **Road Name** | **Road Length** | **Approved Rate Paver block** | **Total Amount** |
| --- | --- | --- | --- | --- |
| 1 | Various locations in Kalyan Division | 130 meters | 9269.27 | 1205005.1 |
| 2 | Land Rent 10rs/pm for 20 years | 130 meters | 200.00 | 226000 |
| 3 | Supervision Charges on RI 15% | - | - | 180750.76 |
| 4 | Security Deposit on RI Charges 10% | - | - | 120500.51 |
|  |  |  | Total | **1532256.37** |

**Total Amount A = Rs -**15,32, 256.37/-

Say Rs. 15,32, 256/-

**Terms and Conditions:**

1. Inform the Police City Traffic Branch, Kalyan before road excavation and carry out the work as per their convenience.
2. While laying the cable, excavate at least 1 foot away from the concrete road edge.
3. Ensure no obstruction or accidents occur during the work.
4. After completing the excavation, refill the dug soil properly and remove the remaining soil to ensure smooth traffic flow.
5. Contact the relevant department before starting the excavation work and begin only with their consent.
6. Notify the Deputy Engineer (Construction Headquarters) before starting the excavation work. Submit a weekly report with photographs to the Deputy Engineer (Construction Headquarters) after starting the work. If the report is unsatisfactory, the permission granted may be revoked.
7. You will be fully responsible for any accidents or loss of life during the excavation.
8. You will be responsible for repairing or compensating for any damage to water pipelines, electrical cables, telephone cables, etc., during the excavation.
9. Display a board with the work details, contractor's name, and contact information at the excavation site.
10. Implement necessary safety measures, such as installing safety tapes, barricades, and name boards indicating the excavation work and company name. Address any complaints promptly, or face penalties.
11. After completing the excavation work, conduct a survey with the Deputy Engineer (Construction Headquarters) and submit a report. If the road length increases, pay the additional excavation fee to the Municipal Corporation.

The total amount proposed for M/s Bharti Airtel Ltd. is Rs. 15,32,256/- (Rupees Fifteen Lakh Thirty Two Thousand Two Hundred Fifty –Six Only), subject to the terms and conditions of the Municipal Corporation.

**Executive Engineer (Construction/Kalyan)**  
Kalyan Dombivli Municipal Corporation, Kalyan Division.

**Copy to:**  
City Engineer, Kalyan Dombivli Municipal Corporation, Kalyan for information.